Safety Annex Users Guide

Version 0.2

Danielle Stewart, University of Minnesota

Janet (Jing) Liu, Rockwell Collins

Darren Coffer, Rockwell Collins  
Mike Whalen, University of Minnesota

Version History

|  |  |  |  |
| --- | --- | --- | --- |
| Version | Date | Author | Information |
| 0.1 | 9/1/2017 | Danielle Stewart | Initial version of the Safety Annex Users Guide. |
|  |  |  |  |
| 0.2 | 3/22/2018 | Danielle Stewart | Updates to tool and grammar |
|  |  |  |  |
|  |  |  |  |

# Table of Contents

[1 Table of Contents 3](#_Toc509396378)

[2 Table of Figures 5](#_Toc509396379)

[3 Introduction 6](#_Toc509396380)

[4 Brief Overview of AADL, AGREE, and the Safety Annex 7](#_Toc509396381)

[4.1 Using the Safety Annex AADL Plugin 10](#_Toc509396382)

[5 Safety Annex Language 17](#_Toc509396383)

[5.1 Syntax Overview 17](#_Toc509396384)

[5.2 Lexical Elements and Types 18](#_Toc509396385)

[5.3 Subclauses 19](#_Toc509396386)

[5.4 Spec Statement 20](#_Toc509396387)

[5.4.1 Fault Statement 21](#_Toc509396388)

[5.4.1.1 Input Statement 21](#_Toc509396389)

[5.4.1.2 Output Statement 22](#_Toc509396390)

[5.4.1.3 Duration Statement 22](#_Toc509396391)

[5.4.1.4 Trigger Statement 23](#_Toc509396392)

[5.4.1.5 Probability Statement 23](#_Toc509396393)

[5.4.1.6 Propagation Type Statement 23](#_Toc509396394)

[5.4.1.7 Safety Equation Statements 23](#_Toc509396395)

[5.4.1.7.1 Eq Statements 24](#_Toc509396396)

[5.4.1.7.2 Set Statements 24](#_Toc509396397)

[5.4.1.7.3 Range Statements 24](#_Toc509396398)

[5.4.1.7.4 Interval Statements 25](#_Toc509396399)

[5.4.2 Analysis Statement 26](#_Toc509396400)

[5.4.2.1 Max N Faults Analysis 26](#_Toc509396401)

[5.4.2.2 Probabilistic Analysis 26](#_Toc509396402)

[5.4.3 Hardware Fault Statement 26](#_Toc509396403)

[5.4.3.1 Duration 27](#_Toc509396404)

[5.4.3.2 Probability 27](#_Toc509396405)

[5.4.3.3 Propagation Type 27](#_Toc509396406)

[6 The Tool Suite (Safety Annex, AGREE, AADL) 28](#_Toc509396407)

[6.1 Tool Suite Overview 28](#_Toc509396408)

[6.2 Installation 29](#_Toc509396409)

[6.2.1 Install OSATE 29](#_Toc509396410)

[6.2.2 Install SMT Solver 31](#_Toc509396411)

[6.2.3 Install JKind Model Checker 33](#_Toc509396412)

[6.2.4 Install AGREE 34](#_Toc509396413)

[6.2.5 Install Safety Annex 37](#_Toc509396414)

# Table of Figures

[Figure 1: Toy Example for Safety Annex and AGREE 8](#_Toc509396424)

[Figure 2: AADL Code for Toy Example with AGREE and Safety Annexes 10](#_Toc509396425)

[Figure 3: Import Menu Option 11](#_Toc509396426)

[Figure 4: Importing Toy Example Project 12](#_Toc509396427)

[Figure 5: Workspace After Importing Toy Example 13](#_Toc509396428)

[Figure 6: AGREE and Safety Analysis Dropdown Menu 14](#_Toc509396429)

[Figure 7:AGREE Verification Results 14](#_Toc509396430)

[Figure 8: Counterexample from Safety Analysis 16](#_Toc509396431)

[Figure 9: Generated Excel File for Counterexample 17](#_Toc509396432)

[Figure 10: Medical Device Example 20](#_Toc509396433)

[Figure 11: Safety Annex Grammar 21](#_Toc509396434)

[Figure 12: Fault Node Definition 22](#_Toc509396435)

[Figure 13: Propagation Statement Example 24](#_Toc509396436)

[Figure 14: Max One Fault Example 27](#_Toc509396437)

[Figure 15: Probability Threshold Example 27](#_Toc509396438)

[Figure 16: Hardware Fault Statement 28](#_Toc509396439)

[Figure 17: Overview of Safety Annex/AGREE/OSATE Tool Suite 30](#_Toc509396440)

[Figure 18: OSATE Loading Screen 31](#_Toc509396441)

[Figure 19: Windows 10 System Control Panel 32](#_Toc509396442)

[Figure 20: System Properties Dialog Box 33](#_Toc509396443)

[Figure 21: Environment Variables Dialog Box 33](#_Toc509396444)

[Figure 22: System Variable Text Edit Box 34](#_Toc509396445)

[Figure 23: OSATE/plugins Directory with .jar Files Replaced 36](#_Toc509396446)

[Figure 24: AGREE Install Test 37](#_Toc509396447)

[Figure 25: SMT Solver Selection 37](#_Toc509396448)

[Figure 26: Safety Analysis Menu Item 38](#_Toc509396449)

# Introduction

System safety analysis techniques are well-established and are a required activity in the development of safety-critical systems. Model-based systems engineering (MBSE) methods and tools based on formal methods now permit system-level requirements to be specified and analyzed early in the development process. While model-based development methods are widely used in the aerospace industry, they are only recently being applied to system safety analysis.

The Safety Annex for the Architecture Analysis and Design Language (AADL) provides the ability to reason about faults and faulty component behaviors in AADL models. In the Safety Annex approach, we use formal assume-guarantee contracts to define the nominal behavior of system components. The nominal model is then verified using the Assume Guarantee Reasoning Environment (AGREE). The Safety Annex provides a way to weave faults into the nominal system model and analyze the behavior of the system in the presence of faults. The Safety Annex also provides a library of common fault node definitions that is customizable to the needs of system and safety engineers.

The Safety Annex supports model checking and quantitative reasoning by attaching behavioral faults to components and then using the normal behavioral propagation and proof mechanisms built into the AGREE AADL annex. This allows users to reason about the evolution of faults over time, and produce counterexamples demonstrating how component faults lead to system failures. It can serve as the shared model to capture system design and safety-relevant information, and produce both qualitative and quantitative description of the causal relationship between faults/failures and system safety requirements.

This Users Guide is organized as follows. Section 2 provides a brief overview of AADL, AGREE, and the Safety Annex. Section 3 gives examples and explanations of the grammar and language of the safety annex. Section 4 provides a detailed approach for the tool suite and downloads.

# Brief Overview of AADL, AGREE, and the Safety Annex

The safety annex is meant to be used in the context of an AADL model that has been annotated with AGREE. AGREE models the components and their connections as they are described in AADL and the safety annex provides fault definitions to these components and connections. This section provides a very brief introduction to AADL, AGREE, and the safety annex through the use of a very simple model.

Suppose we have a simple architecture with three subcomponents A, B, and C, as shown in Figure 1.



Figure 1: Toy Example for Safety Annex and AGREE

We want to show using AGREE that the system level property (Output < 50) holds, given the guarantees provided by the components and the system assumption (Input < 10). We also want to be able to model faults on each of these components. Some possible faults are shown in the diagram of Figure 1.

In order to represent this model in AADL, we construct an AADL package. Packages are the structuring mechanism in AADL; they define a namespace where we can place definitions. We define the subcomponents first, then the system component. The complete AADL is shown in Figure 2 below.

**package** Integer\_Toy

**public**

**with** Base\_Types;

**with** faults;

**system** A

**features**

Input: **in** **data** **port** Base\_Types::Integer;

Output: **out** **data** **port** Base\_Types::Integer;

**annex** agree {\*\*

**assume** "A input range" **:** Input **<** 20**;**

**guarantee** "A output range" **:** Output **<** 2**\***Input**;**

\*\*};

**annex** safety {\*\*

**fault** stuck\_at\_fault\_A "Component A output stuck" **:** faults**.**fail\_to **{**

**inputs:** val\_in **<-** Output**,** alt\_val **<-** **prev(**Output**,** 0**);**

**outputs:** Output **<-** val\_out**;**

**probability:** 5.0E-5 **;**

**duration:** **permanent;**

**}**

\*\*};

**end** A ;

**system** B

**features**

Input: **in** **data** **port** Base\_Types::Integer;

Output: **out** **data** **port** Base\_Types::Integer;

**annex** agree {\*\*

**assume** "B input range" **:** Input **<** 20**;**

**guarantee** "B output range" **:** Output **<** Input **+** 15**;**

\*\*};

**annex** safety {\*\*

**fault** stuck\_at\_fault\_B "Component B output stuck nondeterministic" **:** faults**.**fail\_to **{**

**eq** nondet\_val **:** **int;**

**inputs:** val\_in **<-** Output**,** alt\_val **<-** nondet\_val**;**

**outputs:** Output **<-** val\_out**;**

**probability:** 5.0E-9 **;**

**duration:** **permanent;**

**}**

\*\*};

**end** B ;

**system** C

**features**

Input1: **in** **data** **port** Base\_Types::Integer;

Input2: **in** **data** **port** Base\_Types::Integer;

Output: **out** **data** **port** Base\_Types::Integer;

**annex** agree {\*\*

**eq** mode **:** **int;**

**guarantee** "mode always is increasing" **:** mode **>=** 0 **->** mode **>** **pre(**mode**);**

**guarantee** "C output range" **:** Output **=** **if** mode **=** 3 **then** **(**Input1 **+** Input2**)** **else** 0**;**

\*\*};

**end** C ;

**system** top\_level

**features**

Input: **in** **data** **port** Base\_Types::Integer;

Output: **out** **data** **port** Base\_Types::Integer;

**annex** agree {\*\*

**eq** mode **:** **int;**

**assume** "System input range " **:** Input **<** 10**;**

**guarantee** "mode is always positive" **:** mode **>=** 0**;**

**guarantee** "System output range" **:** Output **<** 50**;**

\*\*};

**end** top\_level;

**system** **implementation** top\_level.Impl

**subcomponents**

A\_sub : **system** A ;

B\_sub : **system** B ;

C\_sub : **system** C ;

**connections**

IN\_TO\_A : **port** Input -> A\_sub.Input

{Communication\_Properties::Timing => immediate;};

A\_TO\_B : **port** A\_sub.Output -> B\_sub.Input

{Communication\_Properties::Timing => immediate;};

A\_TO\_C : **port** A\_sub.Output -> C\_sub.Input1

{Communication\_Properties::Timing => immediate;};

B\_TO\_C : **port** B\_sub.Output -> C\_sub.Input2

{Communication\_Properties::Timing => immediate;};

C\_TO\_Output : **port** C\_sub.Output -> Output

{Communication\_Properties::Timing => immediate;};

**annex** agree{\*\*

**assign** mode **=** C\_sub**.**mode**;**

\*\*};

**annex** safety{\*\*

**analyze** **:** **probability** 1.0E-7

--analyze : max 1 fault

\*\*};

**end** top\_level.Impl;

toy1

Figure 2: AADL Code for Toy Example with AGREE and Safety Annexes

In Figure 2, **system**s define hierarchical "units" of the model. They communicate over **port**s**,** whichare typed. Systems do not contain any internal structure, only the interfaces for the system.

A **system** **implementation** describes an implementation of the system including its internal structure. For this example, the only system whose internal structure is known is the "top level" system, which contains subcomponents A, B, and C. We instantiate these subcomponents (using A\_sub, B\_sub, and C\_sub) and then describe how they are connected together. In the connections section, we must describe whether each connection is *immediate* or *delayed.* Intuitively, if a connection is *immediate,* then an output from the source component is *immediately* available to the input of the destination component (i.e., in the same frame). If they are *delayed*, then there is a one-cycle delay before the output is available to the destination component (delayed frame).

**Note:** Top level analysis can be performed only within a system implementation.

After the AGREE annexes are added to each of the components in the model and verification is complete, the safety annexes can be added to each of the components.

**Important Note: At this time, fault hypotheses (see Figure 3) must be added to each layer of a system in order for analysis to proceed correctly. Also, at most one of the analysis statements must be present. In the example shown in Figure 3, the maximum *n* faults analysis statement is commented out. In this case, the probabilistic analysis will be run.**



Figure 3: Fault Hypothesis Example

## Using the Safety Annex AADL Plugin

The example project used in the rest of this section can be retrieved from the following link:

<https://github.com/loonwerks/AMASE/tree/develop/examples>. Assuming the necessary tools are installed (see section 6), the model can be imported by choosing File > Import:



Figure 4: Import Menu Option

Then choosing "Existing Project into Workspace."



Figure 5: Importing Toy Example Project

and navigate to the unzipped directory after pressing the Next button. Figure 5 shows what the model looks like when loaded in the AGREE/OSATE tool. The project that we are working with is called Toy\_Example\_Safety.



Figure 6: Workspace After Importing Toy Example

Open the Integer\_Toy.aadl model by double-clicking on the file in the AADL Navigator pane. To invoke the safety analysis, we select the Top\_Level.Impl system implementation in the outline pane on the right. We then select “Safety Analysis” in the menu and then run AGREE. We can choose “AGREE > Verify Single Layer” from the AGREE menu as shown in Figure 6.



Figure 7: AGREE and Safety Analysis Dropdown Menu

As AGREE runs, you should see checks for “Contract Guarantees”, ”Contract Assumptions”, and “Contract Consistency” as shown in Figure 7.



Figure 8:AGREE Verification Results

If “Safety Analysis” was checked by the user, this will run the analysis and will change the AGREE contracts accordingly.

When a property fails in AGREE, there is an associated counterexample that demonstrates the failure. To see the counterexample, right-click the failing property (in this case: "System output range") and choose "View Counterexample in Console" to see the values assigned to each of the variables referenced in the model. Figure 8 shows the counterexample that is generated by this failure in the console window given one permanent fault in the system.

It is worth noting in the counterexample of Figure 8 that the faults assigned to components A and B are listed as “Component A output stuck” and “Component B output stuck nondeterministic.” These are the strings assigned to the fault definitions from Figure 2.

It is also possible that each fault has a probability of occurrence. In the Toy Example safety annexes, an arbitrary probability is assigned to each fault for the illustrative purposes. A top level probabilistic threshold is assigned. Assuming independence of faults, safety analysis proceeds by determining if there are sets of faults that will cause the system to fail given this threshold. Figure 7 shows the analysis of the Toy Example given a top level probability threshold of 1.0E-7. The reason this passes the threshold is due to the fact that the most problematic of the faults is with component B (nondeterministic failure) and the probability of component B fault is 1.0E-9. This is beyond the threshold assigned at the lower level.



Figure 9: Counterexample from Safety Analysis

For working with complex counterexamples, it is often necessary to have a richer interface. It is also possible to export the counterexample to Excel by right-clicking the failing property and choosing "View Counterexample in Excel". **Note: In order to use this capability, you must have Excel installed on your computer. Also, you must associate .xls files in Eclipse with Excel.** To do so, the following steps can be taken:

1. Choose the "Preferences" menu item from the Window menu, then
2. On the left side of the dialog box, choose General > Editors > File Associations, then
3. Click the "Add…" button next to "File Types" and then
4. Type "\*.xls" into the text box.

The .xls file type should now be selected.

1. Now choose the "Add…" button next to "Associated Editors"
2. Choose the "External Programs" radio button
3. Select "Microsoft Excel Worksheet" and click OK.

The generated Excel file for the example is shown in Figure 9.



Figure 10: Generated Excel File for Counterexample

# Safety Annex Language

In this chapter we present the syntax and semantics of the input language of the Safety Annex. We refer readers to the AGREE Users Guide for a thorough description of lexical elements, types, and other syntactical details.

## Syntax Overview

Before describing the details of the language, we provide some general notes about the syntax. productions enclosed in parentheses (‘()’) indicate a set of choices in which a vertical bar (‘|’) is used to separate alternatives in the syntax rules. Any characters in single quotes describe concrete syntax (e.g. ‘←’, ‘;’, ‘:’). Examples of grammar fragments are also written in the Courier font. Sometimes one of the following characters is used at the beginning of a rule as a shorthand for choosing among several alternatives:

1) The \* character indicates repetition: zero or more occurrences and the + character indicates required repetition: one or more occurrences.

2) A ? character indicates that the preceding token is optional.

The Safety Annex is built on top of the AADL 2.0 architecture description language as well as the AGREE language. The Safety Annex formulas are found in an AADL annex which extends the grammar of both AADL and AGREE. Generally, the annex follows the conventions of AADL in terms of lexical elements and types with some small deviations (which are noted in the AGREE Users Guide). The Safety Annex operates over a relatively small fragment of both AADL syntax and AGREE syntax. We will not build up the language starting from the smallest fragments, but instead refer the user to the AGREE Users Manual.

AADL describes the interface of a component in a *component type*. A *component type* contains a list of *features* that are inputs and outputs of a component and possibly a list of AADL properties. A *component implementation* is used to describe a specific instance of a *component type*. A *component implementation* contains a list of subcomponents and a list of connections that occur between its subcomponents and features.

The syntax for a component’s contract exists in an AGREE annex placed inside of the *component type*. AGREE syntax can also be placed inside of annexes in a *component implementation* or an AADL package. Syntax placed in an annex in an AADL package can be used to create libraries that can be referenced by other components.

The syntax for a component’s faults exists in a Safety annex placed inside of the *component type* as well. Safety syntax can also be placed inside of annexes in a *component implementation*. This annex links directly to the AGREE annex also associated with the component in question.

## Lexical Elements and Types

For a more thorough description of lexical elements and types, we refer to the AGREE User Guide. Here is a brief description of commonly used lexical elements.

Comments always start with two adjacent hyphens and span to the end of the line. Here is an example:

-- Here is a comment.

-- a long comment may be split onto

-- two or more consecutive lines

An identifier is defined as a letter followed by zero or more letters, digits, or single underscores:

ID ::= identifier\_letter ( ('\_')? letter\_or\_digit)\*

letter\_or\_digit ::= identifier\_letter | digit

identifier\_letter ::= ('A'..'Z' | 'a'..'z')

digit ::= (0..9)

Some example identifiers are: count, X, Get\_Name, Page\_Count. **Note: Identifiers are case insensitive.** Thus Hello, HeLlo, and HELLO all refer to the same entity in AADL.

Boolean and numeric literal values are defined as follows:

Literal :: = Boolean\_literal | Integer\_literal | Real\_literal

Integer\_literal ::= decimal\_integer\_literal

Real\_literal ::= decimal\_real\_literal

decimal\_integer\_literal ::= ('–')? numeral

decimal\_real\_literal ::= ('–')? numeral '.' numeral

numeral ::= digit\*

Boolean\_literal are: true, false.

Examples of Integer\_literals are: 1, 31, -1053

Examples of Real\_literals are: 3.1415, 0.005, 7.01

String elements are defined with the following syntax:

STRING ::= "(string\_element)\*"

string\_element ::= "" | non\_quotation\_mark\_graphic\_character

Primitive data types (bool, int, real) have been built into the AGREE language and are hence part of the Safety annex language. For more information on types, see the AGREE Users Guide.

Safety annex requires reasoning about AADL Data Implementations. Consider the following example from a model of a medical device:

**data** Alarm\_Outputs

**end** Alarm\_Outputs;

**data** **implementation** Alarm\_Outputs.Impl

**subcomponents**

Is\_Audio\_Disabled : **data** Base\_Types::Boolean;

Notification\_Message : **data** Base\_Types::Integer ;

Log\_Message\_ID : **data** Base\_Types::Integer ;

**end** Alarm\_Outputs.Impl;

**placeholder**

Figure 11: Medical Device Example

One can reference the fields of a variable type *Alarm\_Outputs.Impl* by placing a dot after the variable:

*Alarm.Is\_Audio\_Disabled*, *Alarm.Notification\_Message*, or *Alarm.Log\_Message\_ID*.

## Subclauses

Safety annex subclauses can be embedded in *system, process,* and *thread* components. Safety subclauses are of the form:

**annex** safety {\*\*

-- safety spec statements here...

\*\*};

From within the subclause, it is possible to refer to the features and properties of the enclosing component as well as the inputs and outputs of subcomponents (if the subclause is a component implementation). A simplified description of the top-level grammar for Safety annex is shown in

SpecStatement: 'fault' ID (STRING)? ':' faultDefName '{' (FaultSubcomponent)\* '}'

| 'analyze' ':' AnalysisBehavior

| ‘hw\_fault ':' ID (STRING)? ':' '{' (HWFaultSubcomponent)\* '}'

| 'propagate\_from' ':' '{' (SourceFaultList) '@' (SourceCompPath) '}'

‘to’ '{' (DestFaultList) '@' (DestCompPath) '}'

AnalysisBehavior: 'max' Int\_Literal 'fault'

| 'probability' Real\_Literal

FaultSubcomponent: 'inputs' ':' NamedID '<-' Expr (','NamedID '<-' Expr)\* ';'

| 'outputs' ':' NestedDotID '<-' NamedID (','NestedDotID '<-' NamedID)\* ';'

| 'duration' ':' TemporalConstraint (Interval)? ';'

| 'probability' ':' Real\_Literal ';'

| 'enabled' ':' TriggerCondition ';'

| 'propagate\_type' ':' PropagationTypeConstraint ';'

| SafetyEqStatement

HWFaultSubcomponent: 'duration' ':' TemporalConstraint (Interval)? ';'

| 'probability' ':' Real\_Literal ';'

| 'propagate\_type' ':' PropagationTypeConstraint ';'

PropagationTypeConstraint: 'asymmetric'

| 'symmetric'

TemporalConstraint: 'permanent'

| 'transient'

TriggerCondition: 'must' '{' Expr ("," Expr)\* '}'

| 'enabler' '{' Expr ("," Expr)\* '}'

SafetyEqStatement: 'eq' (Arg (',' Arg)\*) ('=' Expr)? ';'

| 'interval' ID '=' Interval ';'

| 'set' ID '=' '{'INTEGER\_LIT (',' INTEGER\_LIT)\* '}' ';'

Interval: '[' Expr ',' Expr ']')

| '(' Expr ',' Expr']')

| '[' Expr ',' Expr ')')

| '(' Expr ',' Expr ')')

**placeholder**

Figure 12: Safety Annex Grammar

A Safety subclause consists of a spec statement which consists of a sequence of statements. These different kinds of statements and their uses are described in section 3.4.

Safety subclauses can occur either within an AADL component or component implementation.

## Spec Statement

The Safety annex subclause can contain one or more spec statements. The following shows the syntax of a spec statement:

SpecStatement: 'fault' ID (STRING)? ':' faultDefName '{' (FaultSubcomponent)\* '}'

| 'analyze' ':' AnalysisBehavior

| ‘hw\_fault ':' ID (STRING)? ':' '{' (HWFaultSubcomponent)\* '}'

| 'propagate\_from' ':' '{' (SourceFaultList) '@' (SourceCompPath) '}'

‘to’ '{' (DestFaultList) '@' (DestCompPath) '}'

Each spec statement corresponds with one fault definition that will wrap a single component. In the case of multiple fault types on a component with multiple outputs, the subclause will contain more than one spec statement; one for each of the fault definitions.

The ID is used as an internal identification to the fault described in the spec statement. The STRING is a description of the fault and will be shown to the user during verification. The fault definition name (a NestedDotID) corresponds with a fault contained in a library of faults. Each of the faults is an AGREE node definition that is placed within an AADL package and included in the component implementation file. These faults can then be referenced by the Safety annex. In the case when the user wishes to design custom faults, refer to the AGREE User Guide description of nodes (3.6.6 Node Definitions).

An example of a fault node is provided:

****

Figure 13: Fault Node Definition

The input and output statements (section 3.5.1, 3.5.2) will refer directly to the inputs and return values of the fault node. Every fault node definition contains an input parameter called trigger\*. All other input parameters are linked in the Inputs statement (section 3.5.1) and the return values are linked with AADL component in the Outputs statement (section 3.5.2).

The fault spec statement will contain zero or more Fault Subcomponent statements. In the case of zero, no faults wrap the AADL component and hence no fault analysis is performed.

\*In future work, this trigger will be linked to the trigger statement shown in the grammar above.

### Fault Statement

The Safety annex spec statement can contain multiple Fault Subcomponent statements. The following is a simplified version of the syntax of a Fault Subcomponent statement:

FaultSubcomponent: 'inputs' ':' NamedID '<-' Expr (','NamedID '<-' Expr)\* ';'

| 'outputs' ':' NestedDotID '<-' NamedID (','NestedDotID '<-' NamedID)\* ';'

| 'duration' ':' TemporalConstraint (Interval)? ';'

| 'probability' ':' Real\_Literal ';'

| 'enabled' ':' TriggerCondition ';'

| 'propagate\_type' ':' PropagationTypeConstraint ';'

| SafetyEqStatement

#### Input Statement

Input statements are where the parameters of the fault node definition are linked to expressions which assign the node parameters a value. Each fault node has a trigger parameter. This is the only input parameter that is not accounted for in the input statement.

As an example, we look at the *fail\_to* fault node definition from Figure 12 and provide an example of the input statement associated with this node.

The inputs that must be explicitly stated are: *val\_in* and *alt\_val*. The left side of the input statement must use these identifiers. The right side of the input statement consists of AGREE or AADL expressions (see AGREE Users Guide, section 3.7). Examples of this include boolean or arithmetic expressions as well as AADL Data Implementation variables. The following is an example of an input statement using the *fail\_to* node and the Toy Example from Figure 2:

**inputs:** val\_in **<-** Output**,** alt\_val **<-** **prev(**Output**,** 0**);**

This input statement will ensure that the value associated with *Output* is passed in as the *val\_in* parameter and likewise the value associated with **prev(**Output**,** 0**)** is the failure value if the fault is triggered (*alt\_val*).

Record types in AADL are supported and their fields can be used in input and output statements.

**Note: The trigger value is not specified within the input statement.** See section 3.5.4 on Trigger Statements.

#### Output Statement

Output statements will specify which component output will be affected by the fault node output. Since nodes may have more than one output, each must be linked to a component. Using the same example in 3.5.1 ( *fail\_to* node and the Toy Example from Figure 2 we describe the associated output statement:

**outputs:** Output **<-** val\_out**;**

In the case of a fault node definition having more than one return value, the output statement would be organized into a list much like the example for input statements in section 3.5.1.

Record types in AADL are supported and their fields can be used in input and output statements.

#### Duration Statement

A duration statement specifies whether the fault will be transient\* or permanent. A permanent fault will remain indefinitely and has no such interval in the statement.

An example of a permanent fault is as follows:

**duration: permanent;**

\*Transient faults are currently not supported in the safety annex. This will be implemented in future work. The only possible faults at this time are permanent.

#### Trigger Statement

The safety annex currently does not support trigger statements. This will be implemented in future work. The following is a description of what trigger statements will look like once implemented.

There are two types of triggers that can occur within a model. We call these *must* triggers and *enabler* triggers. The *must* triggers are of the form: if the trigger has occurred, then the fault must have been activated. The *enabler* triggers are of the form: if the trigger has occurred, then the fault may have been activated. In either of these cases, the triggers are specified using a list or a series of disjunctions. The trigger may have a probability associated with it. This probabilistic value is an optional piece of the statement. The following is a simplified grammar of the trigger statement syntax:

TriggerCondition: 'must' '{' Expr ("," Expr)\* '}'

| 'enabler' '{' Expr ("," Expr)\* '}'

#### Probability Statement

#### Propagation Statement

Users can specify fault dependencies outside of fault statements, typically in the system implementation where the system configuration that causes the dependencies becomes clear (e.g., binding between SW and HW components, co-location of HW components). This is because fault propagations are typically tied to the way components are connected or bound together; this information may not be available when faults are being specified for individual components. Having fault propagations specified outside of a component’s fault statements also makes it easier to reuse the component in different systems. An example of a fault dependency specification is shown in Figure 14, showing that the *valve\_failed* fault at the shutoff subcomponent triggers the *pressure\_fail­\_blue* fault at the selector subcomponent.

****

Figure 14: Propagation Statement Example

#### Safety Equation Statements

To allow flexibility in assigning failure values, various kinds of equation statements are defined for the Safety Annex. This extends the AGREE equation statement by adding three new kinds of equations.

##### Eq Statements

A Safety Equation Statement is identical to an AGREE Equation Statement. Equation statements can be used to create local variable declarations within the body of an AGREE subclause or within a Safety annex fault statement. An example of an equation statement is:

**eq** mode **:** **int** = 9**;**

In this example, we create an integer variable with the value of 9. Variables defined with equation statements can be thought of as ''intermediate'' variables or variables that are not meant to be visible in the architectural model (unlike component outputs or inputs). Equation statements can define variables explicitly by setting the equation equal to an expression immediately after it is defined. Equation statements can also define variables implicitly by not setting them equal to anything. This would capture complete nondeterminism for fault values. An example of this is:

**eq** mode **:** **int;**

To use a nondeterministic value within a fault statement, the equation statement would be defined as above and then used in the input statement to link with the fault node.

Equation statements can define more than one variable at once by writing them in a comma delimited list. One might do this to constrain a list of variables to the results of a node statement that has multiple return values or to more cleanly list a set of implicitly defined variables.

##### Set Statements

Set equation statements are currently not supported in the safety annex. They will be implemented in future work.

Set equation statements can be used to specify a set of discrete values of nondeterminism.

**set** set\_values **= {**0**,**3**,**5**} ;**

The variable set\_values will hold the value 0, 3, or 5.

##### Range Statements

Range equation statements are currently not supported in the safety annex. They will be implemented in future work.

A range equation statement is used to specify a discrete range of integer values. This is the same idea as a set, but is used when the size of the set gets to be unwieldy.

**range** range\_values **= {**0**,**50**} ;**

The variable range\_values will hold some integer value from 0 to 50 inclusive.

##### Interval Statements

Interval equation statements are currently not supported in the safety annex. They will be implemented in future work.

Interval equation statements can be used to specify a real interval of nondeterminism for some variable. These intervals can be any combination of open, closed, or neither. The following is an example of a range including -1.2 up to (but not including) 30.0.

**interval** input\_values **=** [-1.2, 30.0)**;**

### Analysis Statement

An analysis statement is given at the top level of the system implementation under analysis. It will specify the type of analysis to perform. Only one type is permitted to be specified for a single analysis run. There are two kinds of analysis that can be requested by the user. Maximum number of faults present in the system or a probabilistic analysis. These are described below.

#### Max N Faults Analysis

As shown in Figure 15, the user can specify the maximum number of active faults in a system. In this way, it can be determined if the system is resilient to a certain number of faults.



Figure 15: Max One Fault Example

#### Probabilistic Analysis

In order for the probabilistic analysis to run, probabilities must be assigned to each fault definition as shown in the Toy Example of Figure 2. The syntax of probabilistic analysis is shown in Figure 16 with a top level threshold of 1.0E-7. For probabilistic fault hypotheses, we are currently developing a sound approach for composition with respect to the top-level fault probability, but our current tool requires monolithic analysis. Due to this fact, when probabilistic analysis is run, the user should select “Monolithic Analysis” from the AGREE dropdown menu. Any compositional (“Verify Single Layer” or “Verify All Layers”) results with probabilistic analysis is not to be trusted.



Figure 16: Probability Threshold Example

### Hardware Fault Statement

Failures in hardware (HW) components can trigger behavioral faults in the software (SW) or system (SYS) components that depend on them. For example, a CPU failure may trigger faulty behavior in threads bound to that CPU. In addition, a failure in one HW component may trigger failures in other HW components located nearby, such as cascading failure caused by a fire or water damage.

Faults propagate in AGREE as part of a system’s nominal behavior. This means that any propagation in the HW portion of an AADL model would have to be artificially modeled using data ports and AGREE behaviors in SW. This is less than ideal as there may not be concrete behaviors associated with HW components. In other words, faulty behaviors mainly manifest themselves on the SW/SYS components that depend on the hardware components.

To better model faults at the system level dependent on HW failures, we have introduced a new fault model element for HW components. In comparison to the basic fault statement, users are not specifying behavioral effects for the HW failures, nor data ports to apply the failure. An example of a model component fault declaration is shown in Figure 13. This example is taken from the Wheel Brake System model found in <https://github.com/loonwerks/AMASE/tree/develop/examples>.

The example shows the failure of a hardware valve component.



Figure 17: Hardware Fault Statement

In addition, users can specify fault dependencies outside of fault statements using propagation statements. For more information on propagation type statements, see section 5.4.1.6.

#### Duration

The duration of a hardware fault is specified within the hardware fault statement. Currently, the safety annex only supports permanent fault durations. Part of the future work includes transient fault durations.

#### Probability

A probability of the fault occurrence is specified using a probability statement. This is shown in Figure 16. For more information on probabilistic analysis, see section 5.4.2.2.

#### Propagation Type

Propagation types are not yet implemented in the Safety Annex. In future work, this capability will be available.

Faults can be propagated either symmetrically or asymmetrically. In the case of asymmetric fault propagation, we have what are also called Byzantine faults. For example, a hardware component supplies signals to *n* different software components in a fan out manner. If a fault occurs in the hardware component, it can propagate to all software components symmetrically or it can propagate asymmetrically to only a subset of those components. This propagation can be specified within a hardware fault statement using the following syntax.

propagate\_type : symmetric;

propagate\_type : asymmetric;

# The Tool Suite (Safety Annex, AGREE, AADL)

In this chapter we present an overview of the Safety Annex/AGREE/OSATE tool suite, followed by installation instructions for the tool suite, and a description of the main features of the tool suite.

**Note:** At the time of writing this document, the most recent version of OSATE 2.3.2 does not support the Safety Annex. Until this is resolved, to use the Safety Annex with OSATE please proceed through the steps outlined in sections 6.2.2, 6.2.3, and then finally section 6.2.6 to install the OSATE Development Environment.

## Tool Suite Overview

Figure 7 shows an overview of the AGREE/OSATE tool suite. As presented in the figure, OSATE is installed as an Eclipse plugin that serves as the IDE for creating AADL models. Both AGREE and the safety annex will run as a plugins inside OSATE that provides both a language (AADL annex to annotate the models with assume-guarantee behavioral contracts in the case of AGREE and an AADL annex to annotate the model with faults in the case of the safety annex) and a tool (for compositional verification of the contracts reside in AADL models). AGREE translates an AADL model and its contract annotations into Lustre and then queries the JKind model checker to perform the verification. JKind invokes a backend Satisfiability Modulo Theories (SMT) solver (e.g., Yices or Z3) to validate if the guarantees are valid in the compositional setting. The safety annex uses an extension point in AGREE to access the AGREE program and insert the faults into the AGREE contracts. Then that program is translated into Lustre and the JKind model checker is queried to perform the verification/safety analysis.



Figure 18: Overview of Safety Annex/AGREE/OSATE Tool Suite

## Installation

Installing the Safety Annex/AGREE/OSATE Tool Suite consists of 5 main steps, described in each of the following sections.

### Install OSATE

Binary releases of the OSATE tool suite for different platforms are available at: <http://www.aadl.info/aadl/osate/stable/>. Choose the most recent version of OSATE that is appropriate for your platform. For example, at the time of writing this document, the most current release of OSATE is 2.3.2, available for download from <http://osate.org/download-and-install.html>.

After following the OSATE download instructions found on the OSATE download site (above) The splash screen shown in Figure 14 should appear, and OSATE should begin loading.



Figure 19: OSATE Loading Screen

If OSATE loads successfully, continue to the next step in the installation process. If not, and you are running Windows, the most likely culprit involves mismatches between the 32-bit and 64-bit version of OSATE and the bit-level of the Windows OS. Please check to see whether the version of OSATE matches the bit-level of your version of Windows OS. If running Windows 10, this information can be found in the System Control Panel as shown below in Figure 15. Note that this information is also required for downloading the correct version of the SMT Solver in the next installation step.



Figure 20: Windows 10 System Control Panel

### Install SMT Solver

Either one of the following SMT solvers can be used as the underlying symbolic solver invoked by the JKind model checker: Yices from SRI, or Z3 from Microsoft, Inc.

To download Yices, navigate to the Yices install page at: <http://yices.csl.sri.com/> and download the version of Yices appropriate for your platform.

To download Z3, navigate to the z3 install page at: <https://github.com/Z3Prover/z3/releases> and download the version of Z3 appropriate for your platform.

Either tool must be unzipped and placed in a directory somewhere in the file system. Then this directory must be added to the system path. For directions on how to add directories to your path, please see <http://stackoverflow.com/questions/14637979/how-to-permanently-set-path-on-linux> for Linux, and see <http://architectryan.com/2012/10/02/add-to-the-path-on-mac-os-x-mountain-lion/#.VszAv_krJph> for Mac OS. In Linux, you must add the path to your config file, usually .bashrc.

To add directories to your system path in Windows, first navigate to the System Control Panel and choose the "Advanced system settings" button on the left side of the panel. The system properties dialog will appear. Choose the "Advanced" tab in the dialog as shown in Figure 16 then click "Environment variables".



Figure 21: System Properties Dialog Box

The environment variables dialog box is shown in Figure 21.



Figure 22: Environment Variables Dialog Box

In order to make the application available to all user accounts choose the PATH environment variable in the "System variables" section and click "Edit…". This will bring up a text edit box, as seen in Figure 12. If the existing path string in the text edit box does not end with a semicolon (‘;’), add a semicolon first, then append the path to the SMT solver’s "bin" directory, and click "OK" on the dialogs. The bin directory for the Yices tool is underneath the main Yices directory, e.g., C:\Apps\ yices-2.4.2-x86\_64-pc-mingw32-static-gmp\yices-2.4.2\bin. The bin directory for the Z3 tool is underneath the main z3 directory, e.g., C:\Apps\z3-4.4.1-x64-win\z3-4.4.1-x64-win\bin.



Figure 23: System Variable Text Edit Box

To test whether Yices has been correctly installed on either Windows or Linux, open up a command prompt window and type: yices --version. A version number for Yices matching the installed version should be displayed.

To test whether z3 has been correctly installed on either Windows or Linux, open up a command prompt window and type: z3 -version. A version number for Z3 matching the installed version should be displayed.

### Install JKind Model Checker

Download the latest release of jKind at: <https://github.com/agacek/jkind/releases> and unzip it into a location in the file system. Place the directory containing jkind.jar on your path using the same technique that was described for installing yices.

To test whether JKind has been successfully installed, open a new command window and type "jkind". You should see something like the following:

usage: jkind [options] <input>

-excel generate results in Excel format

-help print this message

-induct\_cex generate inductive counterexamples

-interval generalize counterexamples using interval analysis

-n <arg> maximum depth for bmc and k-induction (default:

200)

-no\_bmc disable bounded model checking

-no\_inv\_gen disable invariant generation

-no\_k\_induction disable k-induction

-pdr\_max <arg> maximum number of PDR parallel instances (0 to

disable PDR)

-read\_advice <arg> read advice from specified file

-scratch produce files for debugging purposes

-smooth smooth counterexamples (minimal changes in input

values)

-solver <arg> SMT solver (default: yices, alternatives: cvc4, z3,

yices2, mathsat, smtinterpol)

-support find a set of support and reduce invariants used

-timeout <arg> maximum runtime in seconds (default: 100)

-version display version information

-write\_advice <arg> write advice to specified file

-xml generate results in XML format

-xml\_to\_stdout generate results in XML format on standard out

C:\apps >

### Install AGREE

Download the latest release of AGREE at: <https://github.com/smaccm/smaccm/releases> and unzip it into a location in the file system. Unzipping the file should create a directory called "plugins" containing a set of .jar files. Then start OSATE if haven’t already, go to Help->Installation Details, and in the "Installed Software" click on AGREE and uninstall the plugin. After uninstall the default AGREE that comes with OSATE, go in to the OSATE/plugins folder and delete the three .jar files that start with "com.rockwellcollins.atc.agree". Then copy all the .jar files from the plugin folder of the AGREE’s latest release into OSATE/plugins folder. Figure 13 shows a screen capture of the OSATE/plugins folder after copying the .jar files that come with AGREE release v2.2.0.0.




Figure 24: OSATE/plugins Directory with .jar Files Replaced

To test whether AGREE has been correctly installed, start OSATE. If it has been correctly installed, an AGREE menu should appear in OSATE, as shown in Figure 14.

**Note**: If Yices version 2.X.X (e.g., 2.4.2) is used, select "Yices 2" in OSATE "Window" menu -> "Preferences" -> "Agree" -> "Analysis" -> SMT Solver, as shown in Figure 15. Users can also adjust the timeout and maximum depth for k-induction to use in the "Analysis" configuration dialog.




Figure 25: AGREE Install Test




Figure 26: SMT Solver Selection

### Install Safety Annex

Download the latest release of the safety annex from: <https://github.com/loonwerks/AMASE/tree/master/safety_annex/plugins> and unzip it into a location in the file system. Unzipping the file should create a directory called “plugins” containing a set of .jar files. Then copy all of the .jar files from the plugin folder of the Safety Annex’s latest release into the OSATE/plugins folder. To test whether the safety annex has been correctly installed, a Safety Annex menu should appear in OSATE as shown in Figure 22.



Figure 27: Safety Analysis Menu Item

At this point, you are ready to import the Toy Example project and begin your own safety analysis.

### Install OSATE Development Environment

Follow the installation directions found at <http://osate.org/setup-development.html>. When all steps are complete, your screen will look like




Figure 28: OSATE Development Environment

The “Other Projects” folder will be empty. Download the latest release of the safety annex from: <https://github.com/loonwerks/AMASE/tree/master/safety_annex/plugins> and unzip it into a location in the file system. Unzipping the file should create a directory called “plugins” containing a set of .jar files. Then copy all of the .jar files from the plugin folder of the Safety Annex’s latest release into the “Other Projects” folder.

To run OSATE, a new Run Configuration must be set up.

Run -> Run configurations…

Then select “Eclipse Applications” from the left menu list and then OSATE2. After naming the configuration and choosing your desired workspace location, select “Run.”

OSATE is set up correctly if you see a configuration similar to the one shown in Figure 27.